--- calo/ground/QLOOK/doc/latex/QL-calo-doc.tex	2005/12/05 16:12:45	1.1.1.1
+++ calo/ground/QLOOK/doc/latex/QL-calo-doc.tex	2006/01/13 10:05:59	1.2
@@ -49,7 +49,8 @@
 % title
 %
 \thispagestyle{empty}
-\title{The Calorimeter Quick--look Output Interpretation}
+%\title{The Calorimeter Quick--look Output Interpretation}
+\title{The Calorimeter Quick--look Operational Manual}
 \author{Emiliano Mocchiutti}
 \maketitle
 \begin{center}
@@ -94,7 +95,7 @@
 {\it \bf STANDARD situations:} \\
 - flat line, in case of a partial RAW data acquisition this is nominal;\\
 - ``no dsp infos'', in case of RAW data acquisition this is nominal;\\
-- more segments not passing through zero is normal behaviour for different runs.
+- more segments not passing through zero is normal behaviour for different runs.\\
 NO ACTIONS to be taken.\\
 {\it \bf NON--STANDARD situations:} \\
 - non linear dependence;\\
@@ -159,7 +160,7 @@
 {\it \bf NOMINAL:}\\
 Most of the data should be inside the yellow region.\\
 {\it \bf STANDARD situations:} \\
-- The distribution spreads over a larger range of ADC values. The file contains calibrations too distant in time or the calorimeter has just been switched on. 
+- The distribution spreads over a larger range of ADC values. The file contains calibrations too distant in time or the calorimeter has just been switched on.\\
 - Signal at about 32000 ADC channels. Latch--up in one or more viwes.\\
 ACTION: check after a calibration, if problem persist contact specialist.\\
 {\it \bf NON--STANDARD situations:} \\
@@ -290,7 +291,7 @@
 {\it \bf Description:}\\
 Baselines (ADC channels) obtained during a calibration procedure.\\
 {\it \bf NOMINAL:}\\
-Most of values inside yellow region.
+Most of values inside yellow region.\\
 {\it \bf STANDARD situations:} \\
 - some hits outside yellow region;\\
 - about six consecutive values at zero or 32000; latch--up alarm from a plane during calibration?\\
